Pressure Reducing Valve.

For effectively reducing water pressure down to a desired working pressure. WRAS Approved.

Max Pressure inlet 16 bar

Adjustable range 1.5 – 6 bar.

Max temperature 60 degrees C.

Set from factory at 3 Bar.



Independent filters are recommended upstream of the valve and the pipe work is fully flushed before installing the valve.

The valve must be protected from frost.

Connections ½” BSP female ( 21mm )

Dimensions.

Length 88 mm. Height 95 mm. Width 50 mm

